<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="72.06" y2="0" width="0" layer="20"/>
<wire x1="72.06" y1="0" x2="72.06" y2="50.79" width="0" layer="20"/>
<wire x1="72.06" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>RST</text>
<text>VCC</text>
<text>D0</text>
<text>D2</text>
<text>D4</text>
<text>D6</text>
<text>D1</text>
<text>D3</text>
<text>D5</text>
<text>D7</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>PORTC</text>
<text>PORTB</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>16</text>
<text>17</text>
<text>18</text>
<text>19</text>
<text>R</text>
<text>G</text>
<text>B</text>
<text>PWR</text>
<text>GND</text>
<text>JTAG/DEBUG</text>
<text>PWR</text>
<text>BLMS</text>
<text>USBDM</text>
<text>3D</text>
<text>team19</text>
</plain>
<libraries>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SM49">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MICRO-FIDUCIAL">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
</package>
<package name="1X08_ROUND">
</package>
<package name="2X4">
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="2X3">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-SMD">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="SWITCH-SPDT">
</package>
</packages>
</library>
<library name="parts">
<packages>
<package name="QFP50P1200X1200X160-64N">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Freescale_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 15:00:11</description>
<packages>
<package name="SOIC127P1030X265-20N">
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOIC127P600X175-14N">
</package>
<package name="SOP50P490X110-10N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12MHZ" library="crystal" package="SM49" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="20MHZ" library="crystal" package="SM49" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C10" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C12" library="SparkFun-Passives" package="EIA3216" value="10uF/10V"/>
<element name="C13" library="SparkFun-Passives" package="0603-CAP" value="470nF"/>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="22uF"/>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="22uF"/>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF"/>
<element name="C6" library="SparkFun-Capacitors" package="0603-CAP" value="36pF"/>
<element name="C7" library="SparkFun-Capacitors" package="0603-CAP" value="36pF"/>
<element name="C8" library="SparkFun-Capacitors" package="0603-CAP" value="18pF"/>
<element name="C9" library="SparkFun-Capacitors" package="0603-CAP" value="18pF"/>
<element name="CAPS" library="SparkFun-Passives" package="EIA3216" value="10uF/10V"/>
<element name="FID1" library="SparkFun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="FID2" library="SparkFun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="FID3" library="SparkFun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="JP1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="CMOS2" library="SparkFun-Connectors" package="AVR_ICSP" value=""/>
<element name="PORTC" library="SparkFun-Connectors" package="1X08_ROUND" value=""/>
<element name="FTDI" library="SparkFun-Connectors" package="1X06" value=""/>
<element name="JP7" library="jumper" package="JP1" value=""/>
<element name="PORTB" library="SparkFun-Connectors" package="1X08_ROUND" value=""/>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="10k"/>
<element name="R10" library="SparkFun-Passives" package="0603-RES" value="47"/>
<element name="R11" library="SparkFun-Passives" package="0603-RES" value="100k"/>
<element name="R12" library="SparkFun-Passives" package="0603-RES" value="47"/>
<element name="R13" library="SparkFun-Passives" package="0603-RES" value="100k"/>
<element name="R14" library="SparkFun-Passives" package="0603-RES" value="680"/>
<element name="R15" library="SparkFun-Passives" package="0603-RES" value="1M"/>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="10k"/>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="1M"/>
<element name="R4" library="SparkFun-Passives" package="0603-RES" value="33"/>
<element name="R5" library="SparkFun-Passives" package="0603-RES" value="33"/>
<element name="R6" library="SparkFun-Passives" package="0603-RES" value="680"/>
<element name="R7" library="SparkFun-Passives" package="0603-RES" value="1k"/>
<element name="R8" library="SparkFun-Passives" package="0603-RES" value="47"/>
<element name="R9" library="SparkFun-Passives" package="0603-RES" value="100k"/>
<element name="RESS" library="SparkFun-Passives" package="0603-CAP" value="100nF"/>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="SWITCH-MOMENTARY-2SMD-REDUNDANT">
<attribute name="PROD_ID" value="SWCH-08247"/>
</element>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$1" library="parts" package="QFP50P1200X1200X160-64N" value="K22F128VLH10"/>
<element name="U$2" library="SparkFun-PowerIC" package="SOT223" value="V_REG_MIC2920"/>
<element name="U$3" library="SparkFun-PowerIC" package="SOT223" value="V_REG_MIC2920"/>
<element name="CMOS1" library="SparkFun-Connectors" package="2X4" value="M04X2"/>
<element name="U1" library="Freescale_By_element14_Batch_1" package="SOIC127P1030X265-20N" value="MC9S08JS16LCWJ">
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="OC_NEWARK" value="14R8903"/>
<attribute name="MPN" value="MC9S08JS16LCWJ"/>
<attribute name="SUPPLIER" value="FREESCALE SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="-"/>
</element>
<element name="U2" library="Texas Instruments_By_element14_Batch_1" package="SOIC127P600X175-14N" value="SN74LV125AD">
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="MPN" value="SN74LV125AD"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="9592504"/>
</element>
<element name="JP9" library="SparkFun-Connectors" package="USB-B-PTH" value="USB-B">
<attribute name="PROD_ID" value="CONN-08278"/>
</element>
<element name="DEBUG" library="SparkFun-Connectors" package="AVR_ICSP" value=""/>
<element name="U4" library="Texas Instruments_By_element14_Batch_1" package="SOP50P490X110-10N" value="TS3USB30EDGSR">
<attribute name="PACKAGE" value="MSOP-10"/>
<attribute name="OC_NEWARK" value="64R0806"/>
<attribute name="MPN" value="TS3USB30EDGSR"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="-"/>
</element>
<element name="LASERS" library="SparkFun-Connectors" package="2X3" value="">
<attribute name="PROD_ID" value="CONN-09701"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="SWITCH-SPDT" value="">
<attribute name="PROD_ID" value="SWCH-08261"/>
</element>
</elements>
<signals>
<signal name="12V_DC">
<contactref element="JP1" pad="PWR"/>
<contactref element="U$2" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="GNDBREAK"/>
<contactref element="JP1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="31"/>
<contactref element="U$1" pad="47"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="CAPS" pad="C"/>
<contactref element="RESS" pad="2"/>
<contactref element="C12" pad="C"/>
<contactref element="C13" pad="2"/>
<contactref element="U1" pad="14"/>
<contactref element="JP7" pad="1"/>
<contactref element="U2" pad="7"/>
<contactref element="C10" pad="2"/>
<contactref element="FTDI" pad="6"/>
<contactref element="FTDI" pad="5"/>
<contactref element="CMOS1" pad="2"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="U$1" pad="16"/>
<contactref element="U$1" pad="15"/>
<contactref element="JP9" pad="GND"/>
<contactref element="DEBUG" pad="8"/>
<contactref element="DEBUG" pad="6"/>
<contactref element="U4" pad="9"/>
<contactref element="U4" pad="5"/>
<contactref element="LASERS" pad="2"/>
<contactref element="LASERS" pad="6"/>
<contactref element="LASERS" pad="4"/>
<contactref element="S3" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="U$3" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="30"/>
<contactref element="U$1" pad="48"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="A"/>
<contactref element="U1" pad="17"/>
<contactref element="U2" pad="14"/>
<contactref element="C10" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="FTDI" pad="4"/>
<contactref element="CMOS1" pad="1"/>
<contactref element="U$1" pad="13"/>
<contactref element="U$1" pad="14"/>
<contactref element="DEBUG" pad="10"/>
<contactref element="U4" pad="10"/>
</signal>
<signal name="VCC5">
<contactref element="U$3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="RESS" pad="1"/>
<contactref element="CAPS" pad="A"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="JP9" pad="VBUS"/>
</signal>
<signal name="EXTAL0">
<contactref element="20MHZ" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U$1" pad="32"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="XTAL0">
<contactref element="20MHZ" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U$1" pad="33"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="SWD_DIO">
<contactref element="U$1" pad="25"/>
<contactref element="R2" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="DEBUG" pad="9"/>
</signal>
<signal name="SWD_CLK">
<contactref element="U$1" pad="22"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="DEBUG" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="C8" pad="1"/>
<contactref element="12MHZ" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="XTAL">
<contactref element="C9" pad="1"/>
<contactref element="12MHZ" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="VSSOSC">
<contactref element="U1" pad="3"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="RESET_B">
<contactref element="U$1" pad="34"/>
<contactref element="R1" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="DEBUG" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="JP9" pad="D+"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="JP9" pad="D-"/>
</signal>
<signal name="USBDP">
<contactref element="U1" pad="16"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="USBDN">
<contactref element="U1" pad="15"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="SWD_I">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="9"/>
<contactref element="U2" pad="8"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="SWD_O">
<contactref element="U1" pad="10"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="SWCLK_O">
<contactref element="U1" pad="11"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="SWD_DRV">
<contactref element="U1" pad="12"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="PTA5">
<contactref element="U1" pad="18"/>
</signal>
<signal name="PTA6">
<contactref element="U1" pad="19"/>
</signal>
<signal name="PTA7">
<contactref element="U1" pad="20"/>
</signal>
<signal name="RSTN_O">
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="BKGD/LED">
<contactref element="U1" pad="6"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="BLMS">
<contactref element="U1" pad="7"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="SWCLK_DRV">
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="SWD_IO">
<contactref element="U2" pad="6"/>
<contactref element="R12" pad="1"/>
<contactref element="U2" pad="10"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="11"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="USB0_DP">
<contactref element="U$1" pad="5"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="USB0_DM">
<contactref element="U$1" pad="6"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="1"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="1"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="USB_SEL">
<contactref element="U4" pad="1"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R14" pad="1"/>
<contactref element="S3" pad="3"/>
</signal>
<signal name="RST_B">
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="FTDI" pad="1"/>
</signal>
<signal name="UART0_RX">
<contactref element="U$1" pad="23"/>
<contactref element="FTDI" pad="3"/>
<contactref element="DEBUG" pad="3"/>
</signal>
<signal name="UART0_TX">
<contactref element="U$1" pad="24"/>
<contactref element="FTDI" pad="2"/>
<contactref element="DEBUG" pad="5"/>
</signal>
<signal name="I2C1_SDA">
<contactref element="U$1" pad="1"/>
<contactref element="CMOS1" pad="4"/>
</signal>
<signal name="I2C1_SCL">
<contactref element="U$1" pad="2"/>
<contactref element="CMOS1" pad="3"/>
</signal>
<signal name="HREF">
<contactref element="CMOS1" pad="6"/>
<contactref element="U$1" pad="54"/>
</signal>
<signal name="XCLK">
<contactref element="CMOS1" pad="8"/>
<contactref element="U$1" pad="56"/>
</signal>
<signal name="VSYNC">
<contactref element="CMOS1" pad="5"/>
<contactref element="U$1" pad="53"/>
</signal>
<signal name="PCLK">
<contactref element="CMOS1" pad="7"/>
<contactref element="U$1" pad="55"/>
</signal>
<signal name="D7">
<contactref element="CMOS2" pad="1"/>
<contactref element="U$1" pad="64"/>
</signal>
<signal name="D4">
<contactref element="CMOS2" pad="4"/>
<contactref element="U$1" pad="61"/>
</signal>
<signal name="D1">
<contactref element="CMOS2" pad="7"/>
<contactref element="U$1" pad="58"/>
</signal>
<signal name="RESET">
<contactref element="CMOS2" pad="9"/>
</signal>
<signal name="D6">
<contactref element="CMOS2" pad="2"/>
<contactref element="U$1" pad="63"/>
</signal>
<signal name="D5">
<contactref element="CMOS2" pad="3"/>
<contactref element="U$1" pad="62"/>
</signal>
<signal name="D0">
<contactref element="CMOS2" pad="8"/>
<contactref element="U$1" pad="57"/>
</signal>
<signal name="PWDN">
<contactref element="CMOS2" pad="10"/>
</signal>
<signal name="D3">
<contactref element="CMOS2" pad="5"/>
<contactref element="U$1" pad="60"/>
</signal>
<signal name="D2">
<contactref element="CMOS2" pad="6"/>
<contactref element="U$1" pad="59"/>
</signal>
<signal name="R_LASER">
<contactref element="U$1" pad="27"/>
<contactref element="LASERS" pad="5"/>
</signal>
<signal name="G_LASER">
<contactref element="U$1" pad="28"/>
<contactref element="LASERS" pad="3"/>
</signal>
<signal name="B_LASER">
<contactref element="U$1" pad="29"/>
<contactref element="LASERS" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="44"/>
<contactref element="PORTC" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="45"/>
<contactref element="PORTC" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="46"/>
<contactref element="PORTC" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="49"/>
<contactref element="PORTC" pad="5"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="50"/>
<contactref element="PORTC" pad="6"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="51"/>
<contactref element="PORTC" pad="7"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="52"/>
<contactref element="PORTC" pad="8"/>
</signal>
<signal name="B0">
<contactref element="U$1" pad="35"/>
<contactref element="PORTB" pad="1"/>
</signal>
<signal name="B1">
<contactref element="U$1" pad="36"/>
<contactref element="PORTB" pad="2"/>
</signal>
<signal name="B2">
<contactref element="U$1" pad="37"/>
<contactref element="PORTB" pad="3"/>
</signal>
<signal name="B3">
<contactref element="U$1" pad="38"/>
<contactref element="PORTB" pad="4"/>
</signal>
<signal name="B16">
<contactref element="U$1" pad="39"/>
<contactref element="PORTB" pad="5"/>
</signal>
<signal name="B17">
<contactref element="U$1" pad="40"/>
<contactref element="PORTB" pad="6"/>
</signal>
<signal name="B18">
<contactref element="U$1" pad="41"/>
<contactref element="PORTB" pad="7"/>
</signal>
<signal name="B19">
<contactref element="U$1" pad="42"/>
<contactref element="PORTB" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="43"/>
<contactref element="PORTC" pad="1"/>
</signal>
<signal name="PTA4">
<contactref element="U$1" pad="26"/>
<contactref element="DEBUG" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="3"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$10">
</signal>
</signals>
</board>
</drawing>
</eagle>
